# CHAPTER-1 INTRODUCTION

## OBJECTIVE:

Security is becoming a crucial component of contemporary warfare Cyberattacks account for the majority of attacks. Cyberattack against Systems, Aircraft, Drones, and other Military Equipment, etc.

The initiative's main objective is to increase data flow, but as time goes on, security issues have taken on more significance. Since cryptography can transform plaintext into cypher and vice versa, its use inside VLSI has lately increased. A large number of HDL modules will be simultaneously written in order to implement the most recent advancements in cryptography technology in the hardware security module. The major goal is to send and receive data securely without allowing data to be hacked, as well as to boost the efficiency of a certain parameter. Verilog code was used as the technique in this system. Analog and digital platforms are offered by Xilinx to support the design of both analogue and digital circuits. Interesting fact: Any encryption algorithm will function.

## Motivation:

The primary goal of the project is to increase system security. To that end, we would use our adaptation of AES encryption to strengthen the hardware security module's security in an environment centered around network-centric warfare. Additionally, to strengthen the security of defense technologies from cyber-attacks.

## Relevance of the project:

Security is becoming a crucial component of contemporary warfare. Cyberattacks account for the majority of attacks. Cyberattack against Systems, Aircraft, Drones, and other Military Equipment, etc. These seriously harm a nation's collateral. In order to achieve our goal of improving system security, we would use our adaptation of AES encryption to strengthen the security of the hardware security module, which is an HSM (Hardware Security Module) chip implanted in the system controller.

# CHAPTER-2 LITERATURE SURVEY

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.NO** | **TITLE** | **AUTHOR** | **PUBLISHED IN** | **INFERENCE** |
| 1 | Journal of Electrical Systems and Information Technology 2  (2015) 178–183 | Power efficient and high performance VLSI  architecture for AES algorithm  K. Kalaiselvi a,∗,  H. Mangalam | **2022** | Advanced encryption standard (AES) algorithm has been widely deployed in cryptographic applications. This work proposes a low  power and high throughput implementation of AES algorithm using key  expansion approach |
| **2** | VLSI  implementarion of AES Algorithm | Surabh Kumar | **2022** | This paper presents In the past cryptography means only encryption and decryption using secret keys, nowadays it is defined in different mechanisms like asymmetric-key  encipherment and |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  | symmetric-key encipherment |
| **3** | VLSI | Favin Fernandes, | **2021** | Through the years, the flow of Data and its transmission have increased tremendously  and so has the security issues to it.  Cryptography  in recent years with the advancement of VLSI has  led to its implementation of Encryption and Decryption techniques, where the process of translating and converting plaintext into cypher  text and vice versa is made possible |
|  | Implementation | Gauravi |  |
|  | of Cryptographic | Dungarwal, |  |
|  | Algorithms | Aishwariya |  |
|  | & Techniques | Gaikwad, Ishan |  |
|  |  | Kareliya, Swati |  |
|  |  | Shilaskar |  |

## CHAPTER-3

**EXISTING AND PROPOSED SYSTEM**

## EXISTING SYSTEM:

Through the years, the flow of Data and its

transmission have increased tremendously and so has the security issues to it. Cryptography in recent years with the advancement of VLSI has led to its implementation of Encryption and Decryption techniques, where the process of translating and converting plaintext into cypher text and vice versa is made possible. In this paper, the review of various aspects of VLSI's implementation of encryption and decryption are covered. Ultimately, with this review, the basic understanding of different VLSI techniques of Encryption and Decryption can be studied and implemented. This is the existing system of the project.

## PROPOSED SYSTEM:

Verilog coding is the method used in this system. We would examine the most recent version of AES encryption first, modify it to reach the algorithm's optimum efficiency, and then implement it in a Hardware Security Module. After that We would implement into a Controller for further study of the Security of the Controller System. This is our proposed methodology of our Project.

## CHAPTER-4 REQUIREMENT SPECIFICATION

* 1. **Hardware requirements:**

## Hardware security module:

A hardware security module (HSM) is a physical computing device that safeguards and manages digital keys, performs encryption and decryption functions for digital signatures, strong authentication and other cryptographic functions. These modules traditionally come in the form of a plug-in card or an external device that attaches directly to a computer or network server. A hardware security module contains one or more secure crypto processor chips.

HSMs may have features that provide tamper evidence such as visible signs of tampering or logging and alerting, or tamper resistance which makes tampering difficult without making the HSM inoperable, or tamper responsiveness such as deleting keys upon tamper detection. Each module contains one or more secure crypto processor chips to prevent tamperingand bus probing, or a combination of chips in a module that is protected by the tamper evident, tamper resistant, or tamper responsive packaging



**Figure 4.1**

## Uses of HSM:

A hardware security module can be employed in any application that uses digital keys. Typically, the keys would be of high value - meaning there would be a significant, negative impact to the owner of the key if it were compromised.

The functions of an HSM are:

* onboard secure cryptographic key generation
* onboard secure cryptographic key storage, at least for the top level and most sensitive keys, which are often called master keys
* key management
* use of cryptographic and sensitive data material, for example, performing decryption or digital signature functions
* offloading application servers for complete asymmetric and symmetric cryptography.

HSMs are also deployed to manage transparent data encryption keys for databases and keys for storage devices suchas disk or tape. HSMs provide both logical and physical protection of these materials, including cryptographic keys, from disclosure, non-authorized use, and potential adversaries. HSMs support both symmetric and asymmetric (public- key) cryptography. For some applications, such as certificateauthorities and digital signing, the cryptographic material is asymmetric key pairs (and certificates) used in public-key cryptography. With other applications, such as data encryption or financial payment systems, the cryptographic material

consists mainly of symmetric keys.



**Figure 4.2**

## 4.1.2 FPGA:

Field Programmable Gate Arrays (FPGAs) are semiconductor devices that are based around a matrix of configurable logic blocks (CLBs) connected via programmable interconnects. FPGAs can be reprogrammed to desired application or functionality requirements after manufacturing. This feature distinguishes FPGAs from Application Specific Integrated Circuits (ASICs), which are custom manufactured for specific design tasks. Although one-time programmable (OTP) FPGAs are available, the dominant types are SRAM based which can be reprogrammed as the design evolves.

14

**Applications:**

* + - * Aerospace & Defense - Radiation-tolerant FPGAs along with intellectual property for image processing, waveform generation, and partial reconfiguration for SDRs.
      * ASIC Prototyping - ASIC prototyping with FPGAs enables fast and accuíate SoCsystem modeling and verification of embedded software
      * Automotive - Automotive silicon and IP solutions foí gateway and device assistance systems, comfort, convenience, and in-vehicle infotainment.
      * Broadcast & AV - Adapt to changing requirements fasted and lengthen product life cycles with Broadcast targeted Design Platforms and solutions for high-end professional broadcast systems.
      * Consumer Electronics - Cost-effective solutions enabling next generation, full- featured consumer applications, such as converged handsets, digital flat panel displays, information appliances, home networking, and residential set top boxes.
      * Data Center - Designed for high-bandwidth, low-latency service, networking, and Storage applications to bring higher value into cloud deployments.
      * High Performance Computing and Data Storage - Solutions for Network Attached Storage (NAS), Storage Area Network (SAN) and storage appliances.
      * Industrial - Xilinx FPGAs and targeted design platforms for Industrial, Scientificand Medical (ISM) enable higher degrees of flexibility, faster time-to-market, andlower overall non-securing engineering costs (NRE) for a wide image of applications such as industrial imaging and surveillance, industrial automation,and medical imaging equipment.
      * Medical - Foí diagnostic, monitoring, and therapy applications, the Vivado FPGA and Spaítan® FPGA families can be used to meet a ímage of processing, display,and I/O interface requirements.
      * Security - Xilinx offers solutions that meet the evolving needs of secuíity applications, from access control to surveillance and safety systems.
      * Video & Image Processing - Xilinx FPGAs and targeted design platforms enable higher degrees of flexibility, faster time-to-market, and lower overall non-securingengineering costs (NRE) for a wide range of video and imaging applications.
      * Wireless Communications - RF, base band, connectivity, transport and networking solutions for wireless equipment, addressing standards such as WCDMA, HSDPA, WiMAX and others.



**Figure 4.3**

## Software Requirements:

* + 1. **VIVADO:**

Vivado is a comprehensive design suite created by AMD for developing and implementing designs on Adaptive SoCs and FPGAs. It offers a variety of tools and features to streamline the entire design flow, from design entry to implementation and verification.

Capabilities:

* + - * Design Input: Vivado supports various design entry formats, including Verilog, VHDL, System Verilog, and IP Integrator.
      * Synthesis: Converts HDL code into a netlist that represents the logic gates and interconnections of your design.
      * Place and Route: Maps the synthesized netlist onto the FPGA fabric, optimizing placement and routing for performance and timing closure.
      * Verification/Simulation: Provides tools for simulating and verifying your design at various levels of abstraction, ensuring its functionality before implementation.
      * System-on-Chip (SoC) Design: Offers advanced features for designing and implementing complex SoC systems, including IP integration, power analysis, and floor planning.
      * High-Level Synthesis (HLS): Enables C/C++ code to be converted into hardware for faster prototyping and design exploration.
      * Timing Closure: Provides a comprehensive set of tools for analyzing and optimizing timing performance, ensuring your design meets timing constraints.
      * Methodology Support: Supports various design methodologies, including Agile, Waterfall, and IP-centric design.

Benefits:

* + - * Improved Productivity: Streamlines the design flow with a unified interface and advanced automation features, leading to faster design cycles.
      * Enhanced Performance: Optimizes designs for performance and timing closure, enabling efficient implementation on FPGAs.
      * Reduced Design Errors: Comprehensive verification tools help identify and eliminate errors early in the design process.
      * Increased Flexibility: Supports various design entry formats and methodologies, offering flexibility for different design styles.
      * IP-Centric Design: Enables efficient integration and reuse of intellectual property (IP) cores, accelerating design creation.



**Figure 4.4**

18


# CHAPTER-5

**ALGORITHM**

# Advanced Encryption Standard:

. The Advanced Encryption Standard (AES) is a symmetric block cipher chosen by the U.S. government to protect classified information.

AES is implemented in software and hardware throughout the world to encrypt sensitive data. It is essential for government computer security, cybersecurity and electronic data protection.



## Figure 5.1

**Working of AES:**

AES includes three block ciphers:

* + - AES-128 uses a 128-bit key length to encrypt and decrypt a block of messages.
    - AES-192 uses a 192-bit key length to encrypt and decrypt a block of messages.
    - AES-256 uses a 256-bit key length to encrypt and decrypt a block of messages.

Each cipher encrypts and decrypts data in blocks of 128 bits using cryptographic keys of 128, 192 and 256 bits, respectively.

Symmetric, also known as secret key, ciphers use the same key for encrypting and decrypting. The sender and the receiver must both know -- and use -- the same secret key.

The government classifies information in three categories: Confidential, Secret or Top Secret. All key lengths can be used to protect the Confidential and Secret level. Top Secret information requires either 192- or 256-bit keylengths.

There are 10 rounds for 128-bit keys, 12 rounds for 192-bit keys and 14 rounds for 256-bit keys. A round consists of several processing steps that include substitution, transposition and mixing of the input plaintext to transform it into the final output of ciphertext.

The AES encryption algorithm goes through multiple rounds of encryption. It can even go through 9, 11, or 13 rounds of this.

Each round involves the same steps below.

* + - Divide the data into blocks.
    - Key expansion.
    - Add the round key.
    - Substitute/replacement of the bytes.
    - Shift the rows.
    - Mix the columns.
    - Add a round key again.
    - Do it all over again.


After the last round, the algorithm will go through one additional round. In this set, the algorithm will do steps 1 to 7 except step 6.

It alters the 6th step because it would not do much at this point. Remember it's already gone through this process multiple times.

So, a repeat of step 6 would be redundant. The amount of processing power it would take to mix the columns again just isn't worth it as it will no longer significantly alter the data.

The AES encryption algorithm defines numerous transformations that are to be performed on data stored in an array. The first step of the cipher is to put the data into an array, after which the cipher transformations are repeated over multiple encryption rounds.

The first transformation in the AES encryption cipher is substitution of data using a substitution table. The second transformation shifts data rows. The third mixes columns. The last transformation is performed on each column using a different part of the encryption key. Longer keys need more rounds to complete



**Figure 5.2**

## Features of AES:

NIST specified the new AES algorithm must be a block cipher capable of handling 128-bit blocks, using keys sized at 128, 192 and 256 bits.

Other criteria for being chosen as the next AES algorithm included the following:


* + - Security. Competing algorithms were to be judged on their ability to resist attack as compared to other submitted ciphers. Security strength was to be considered the most important factor in the competition.
    - Cost. Intended to be released on a global, nonexclusive and royalty-free basis, the candidate algorithms were to be evaluated on computational and memory efficiency.
    - Implementation. Factors to be considered included the algorithm's flexibility, suitability for hardware or software implementation, and overall simplicity.

## Difference between AES encryption and DES encryption:

DES served as the linchpin of government cryptography for years until 1999, when researchers broke the algorithm's 56-bit key using a distributed computer system. In 2000, the U.S. government chose to use AES to protect classified information. DES is still used in some instances for backward compatibility.

The two standards are both symmetric block ciphers, but AES is more mathematically efficient. The main benefit of AES lies in its key length

options. The time required to crack an encryption algorithm is directly related to the length of the key used to secure the communication -- 128-bit, 192-bit or 256-bit keys. Therefore, AES is exponentially stronger than the 56-bit key of DES. AES encryption is also significantly faster, so it is ideal for applications, firmware and hardware that require low latency or high throughput.




**Figure**

# AES 256 Encryption:


we know that these encryption algorithms scramble the information it's protecting and turn it into a random mess.

I mean, the basic principle of all encryption *is* each unit of data will be replaced by a different one, depending on the security key.




**Figure 5.4**

There are several rounds in this encryption process,



**Figure 5.5**


**Add Round Key**: You pass the block data stored in the state array through an XOR function with the first key generated (K0). It passes the resultant state array on as input to the next step.






**Figure 5.6**

**Sub-Bytes**: In this step, it converts each byte of the state array into hexadecimal, divided into two equal parts. These parts are the rows and columns, mapped with a substitution box (S-Box) to generate new values for the final state arra




**Figure 5.7**

**Shift Rows**: It swaps the row elements among each other. It skips the first row. It shifts the elements in the second row, one position to the left. It also shifts the elements from the third row two consecutive positions to the left, and it shifts the last row three positions to the left.




**Figure 5.8**

**Mix Columns**: It multiplies a constant matrix with each column in the state array to get a new column for the subsequent state array. Once all the columns are multiplied with the same constant matrix, you get your state array for the next step. This particular step is not to be done in the last round.




**Figure 5.9**

**Add Round Key**: The respective key for the round is XOR’d with the state array is obtained in the previous step. If this is the last round, the resultant state array becomes the ciphertext for the specific block; else, it passes as the new state array input for the next round.



**Figure 5.10**




**Figure 5.11**

27

As you can see in the image above, the plaintext and encryption convert keys to hex format before the operations begin. Accordingly, you can generate the keys for the next ten rounds, as you can see below

You need to follow the same steps explained above, sequentially extracting the state array and passing it off as input to the next round. The steps are as follows,


Add round key,






**Figure 5.12**

Sub-Bytes: It passes the elements through a 16x16 S-Box to get a completely new state array




**Figure 5.13**

Shift rows,




**Figure 5.14**

Mix columns,




**Figure 5.15**

Add round key,



**Figure 5.16**

This state array is now the final ciphertext for this particular round. This becomes the input for the next round. Depending on the key length, you repeat the above steps until you complete round 10, after which you receive the final ciphertext.



**Figure 5.17**

## Application of AES:


* + - Wireless Security: Wireless networks are secured using the Advanced Encryption Standard to authenticate routers and clients. Wi-Fi networks have firmware software and complete security systems based on this algorithm and are now in everyday use.
    - Encrypted Browsing: AES plays a huge role in securing website server authentication from both client and server end. With both symmetric and asymmetric encryption being used; this algorithm helps in SSL/TLS encryption protocols to always browse with the utmost security and privacy.
    - General File Encryption: Apart from corporate necessities, AES is also used to transfer files between associates in an encrypted format. The encrypted information can extend to chat messages, family pictures, legal documents.
    - Processor Security: Many processor manufacturers enable hardware- level encryption using the likes of AES encryption to bolster security and prevent meltdown failures, among other low-profile risks

**CHAPTER – 6**

**POWER AND LUT ANALYSIS**

## POWER ANALYSIS


our project's success in reducing power consumption compared to existing standards is a testament to our commitment to innovation, efficiency, and sustainability. By embracing advanced technologies, implementing optimized design methodologies, and prioritizing power efficiency throughout the development process, we have achieved remarkable reductions in energy consumption with far-reaching implications for cost savings, environmental preservation, and market competitiveness. As we continue to push the boundaries of power efficiency in our projects, we remain steadfast in our commitment to driving positive change and shaping a more sustainable future.



**Figure 6.1**

## LUT ANALYSIS

The strategic integration of LUT optimization techniques within our project represents a pivotal milestone in our pursuit of efficiency and performance excellence. By harnessing the power of LUTs, we have unlocked new realms of computational efficiency, performance enhancement, and scalability, propelling our project towards unprecedented levels of success. As we continue to innovate and refine our approach, we remain committed to leveraging cutting-edge technologies to drive positive change and deliver value to stakeholders.




32

**Figure 6.2**


# Encryption:

**CHAPTER – 7 EXPERIMENTS OUTPUTS**



# Decryption:

**Figure 7.1**



**Figure 7.2**

33

# CHAPTER – 8 CONCLUSION AND FUTURE SCOPE

## Conclusion:

This leads us to the conclusion that this project might have

research on the definition of cryptography, the AES encryption algorithm, and Xilinx software. From this study, we would modify the AES Encryption algorithm in the best way possible and implement it in the FPGA kit.


## Future scope:

We intended to enhance this project by using an FPGA kit to implement the optimal algorithm in the circuit. Embed this in a controller so that we could check the controller's security and create a commercial product. the DRDO will receive this for integration into their weapon.

34

**APPENDICES A**

**PROOF FOR PUBLICATION**



35

**APPENDICES B**

**ACHIEVEMENTS**

**INNOVATHON 1.0 FINALISTS**








36

**SOLVEATHON 1.0 WINNER**



**COURSES**

****

37

## REFERENCES

1. Kumar, Pramod, T. V. Narendra, and N. A. Vinay. "Short Hand Recognition using Canny Edge Detector." International Journal 7, no. 5 (2017).
2. Kumar, Mamatha MS Pramod, and M.Mamatha. "FPGAImplementation Of Low Area Single Precision Floating Point Multiplier."International Journal of Science Technology and Engineering, Vol.2, no. 2 (2016): 560-566.
3. M.Natheera Banu, FPGA Based Hardware Implementation of Encryption Algorithm, International Journal of Engineering and Advanced Technology (IJEAT) ISSN: 2249 8958, Volume-3, Issue-4, April 2014.
4. Deguang Le, Jinyi Chang, Xingdou Gou, Ankang Zhang ,Conglan Lu

, Parallel AES Algorithm for Fast Data Encryption on GPU, IEEE journal on AES 2010.

1. K. Xinmiao Zhang, High speed VLSI architectures for the AES algorithm, IEEE transactions on VLSI systems, Tech. Rep., sep2004.
2. National Institute of Standards and Technology, Advanced Encryption Standard, Federal Information Processing Standards 197, November 2001.
3. M.Pitchaiah, Philemon Daniel, Praveen, Implementation of Advanced Encryption Standard Algorithm, International Journal of Scientific Engineering Research.

38